**Repeat Mode Setting**

**Version 1.0**

**Version History**

|  |  |  |  |
| --- | --- | --- | --- |
| **Version** | **Date** | **Handled by** | **Comments** |
| V1.0 | 16-Sep-2019 | ZL Chen | First version release. |
|  |  |  |  |

Precondition Setting:

N/A


Please follow the installation steps as below:

Step 1:

Make sure the main AP is launched and should be worked. (RT-AC55U)

SSID: ASUS\_AP\_2.4G

Password: ad20151225



Step 2:

Log in to the RT-AC55U.


Username: admin

Password: 12345678

Step 3:


Add the manual IP’s DHCP list.

LAN -> DHCP Server.



Step 4:

Add the New device as the screenshot.




IP: 192.168.50.111, MAC: 4C:ED:FB:A4:54:58 (RT-AC68U)

IP: 192.168.50.196, MAC: 40:B0:76:37:BC:78 (RT-AC68U)

Step 5:

Please clear all of the known networks.



Step 6:

Attach the AP (192.168.50.111 or 192.168.50.196)





Step 7:

Reset the “Repeat Mode”.









Step 8:

Find the main AP RT-AC55U, then attach it.







Step 9:

Set the wireless network.



Please set the SSID and Password.

(2.4G) SSID: siot\_dqa, Password: ad20151225

(5G) SSID: siot\_dqa\_5g, Password: ad20151225



Then please removal the WAN Ethernet.